Documentation

**Python Driver**

**Position Servo**

Int Set Position Servo (Serial Number , Port Number , Position value)

Serial Number – A,B,C

Port Number – 1,2,3,4

Position Value – 0 – 180

Return:

0 – Unsuccessful do not sure about the reason

1 – Successfully written

2 – No device connected

3 – No adapter connected

**Rotational Servo**

**RGB LEDs**

**Single color LED**